**GET /{appInstanceId}/ue\_identity\_tag\_info**

|  |  |
| --- | --- |
| Description | If none of the parameters are passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-001** |
| **Test Purpose** | Check response received from server when all parameter is null |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{ }/ue\_identity\_tag\_info?ueIdentityTag={ } |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation without specifying any parameters |
|  | |
| **Expected Response code and Message** | 400 Bad Request |
| **Expected Response Example Value** | {  "ProblemDetails": {  "type": "string",  "title": "string",  "status": 0,  "detail": "string",  "instance": "string"  }  } |

**PARAMETER – APPINSTANCEID – 200**

|  |  |
| --- | --- |
| Description | If valid appInstanceId is passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-002** |
| **Test Purpose** | Check response received from server when appInstanceId is valid |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{***Valid\_appInstanceId***}/ue\_identity\_tag\_info?  ueIdentityTag={ueIdentityTag} |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation by specifying valid appInstanceId |
|  | |
| **Expected Response code and Message** | 200 Success |
| **Expected Response Example Value** | {  "UeIdentityTagInfo": {  "ueIdentityTags": [  {  "ueIdentityTag": "UeTagA",  "state": "REGISTERED"  }  ]  }  } |

**PARAMETER – APPINSTANCEID – 400**

|  |  |
| --- | --- |
| Description | If appInstanceId is not passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-003** |
| **Test Purpose** | Check response received from server when appInstanceId is null |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{ }/ue\_identity\_tag\_info?ueIdentityTag={ueIdentityTag} |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation without specifying appInstanceId |
|  | |
| **Expected Response code and Message** | 400 Bad Request |
| **Expected Response Example Value** | {  "ProblemDetails": {  "type": "string",  "title": "string",  "status": 0,  "detail": "string",  "instance": "string"  }  } |

**PARAMETER – APPINSTANCEID – 404**

|  |  |
| --- | --- |
| Description | If invalid appInstanceId is passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-004** |
| **Test Purpose** | Check response received from server when appInstanceId is incorrect |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{***Invalid\_appInstanceId***}/ue\_identity\_tag\_info?  ueIdentityTag={ueIdentityTag} |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation by specifying invalid appInstanceId |
|  | |
| **Expected Response code and Message** | 404 Not Found |
| **Expected Response Example Value** | {  "ProblemDetails": {  "type": "string",  "title": "string",  "status": 0,  "detail": "string",  "instance": "string"  }  } |

**PARAMETER – UEIDENTITYTAG – 200**

|  |  |
| --- | --- |
| Description | If valid ueIdentityTag is passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-005** |
| **Test Purpose** | Check response received from server when ueIdentityTag is valid |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{appInstanceId}/ue\_identity\_tag\_info?  ueIdentityTag={ ***Valid\_ueIdentityTag***} |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation by specifying ueIdentityTag |
|  | |
| **Expected Response code and Message** | 200 Success |
| **Expected Response Example Value** | {  "UeIdentityTagInfo": {  "ueIdentityTags": [  {  "ueIdentityTag": "UeTagA",  "state": "REGISTERED"  }  ]  }  } |

**PARAMETER – UEIDENTITYTAG – 400**

|  |  |
| --- | --- |
| Description | If ueIdentityTag is not passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-006** |
| **Test Purpose** | Check response received from server when ueIdentityTag is null |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{appInstanceId}/ue\_identity\_tag\_info?ueIdentityTag={ } |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation without specifying ueIdentityTag |
|  | |
| **Expected Response code and Message** | 400 Bad Request |
| **Expected Response Example Value** | {  "ProblemDetails": {  "type": "string",  "title": "string",  "status": 0,  "detail": "string",  "instance": "string"  }  } |

**PARAMETER – UEIDENTITYTAG – 404**

|  |  |
| --- | --- |
| Description | If invalid ueIdentityTag is passed |
| **Identifier** | **MEC-MP1-UEIDTAGINFO-007** |
| **Test Purpose** | Check response received from server when ueIdentityTag is incorrect |
| **Configuration** |  |
| **References** | https://forge.etsi.org/rep/gitweb.cgi/MEC.GS\_014.git/tree |
| **Request** | /ui/v1/{appInstanceId}/ue\_identity\_tag\_info?  ueIdentityTag={***Invalid\_ueIdentityTag*** } |
| Applicability |  |
|  | |
| **Pre-test Conditions** | MEC installed and working |
|  | |
| **Test Sequence** | Request list of all bandwidth allocation by specifying invalid ueIdentityTag |
|  | |
| **Expected Response code and Message** | 404 Not Found |
| **Expected Response Example Value** | {  "ProblemDetails": {  "type": "string",  "title": "string",  "status": 0,  "detail": "string",  "instance": "string"  }  } |